---
title: "Load and plot data from Nevada Geodetic Laboratory"
output: rmarkdown::html_vignette
vignette: >
  %\VignetteIndexEntry{Load and plot data from Nevada Geodetic Laboratory}
  %\VignetteEngine{knitr::rmarkdown}
  %\VignetteEncoding{UTF-8}
---

```{r setup, include=FALSE}
knitr::opts_chunk$set(
  fig.width = 10, # Set default plot width (adjust as needed)
  fig.height = 8, # Set default plot height (adjust as needed)
  fig.align = "center" # Center align all plots
)


# knitr::opts_chunk$set(eval = FALSE)
```



Let us first load the `gmwmx2` package.
```{r}
library(gmwmx2)
```

# Download all available stations from NGL

```{r}
all_stations <- download_all_stations_ngl()
head(all_stations)
```

# Download one station
```{r}
data_1LSU <- download_station_ngl("1LSU")
```
# Extract GNSS position time series of station
```{r}
attributes(data_1LSU)
head(data_1LSU$df_position)
```

# Extract equipment or software changes steps
```{r}
head(data_1LSU$df_equipment_software_changes)
```

# Extract earthquakes steps
```{r}
head(data_1LSU$df_earthquakes)
```



# Plot GNSS position time series 
```{r}
plot(data_1LSU)
plot(data_1LSU, component = "N")
plot(data_1LSU, component = "E")
plot(data_1LSU, component = "V")
```
