# Trip planning with detailed_itineraries()

#### 2026-05-19

Abstract

This vignette shows how to do route planning using the `detailed_itineraries()` function in r5r.

# 1. Introduction

r5r has some extremely efficient functions to run multimodal routing and accessibility analysis. In general, though, these functions output only the essential information required by most transport planning applications and simulation models. Moreover, the algorithms behind these function return only the optimal route in terms of minimizing travel times and/or monetary costs. Sometimes, though, we would like to do more simple route planning analysis and extract more information for each route. Also, we might be interested in finding not only the fastest route but some other suboptimal route alternatives too.

This is where the `detailed_itineraries()` function comes in. This function outputs for each origin destination pair a detailed route plan with information per leg, meaning a route taken by a single mode such as a walk to the bus stop. In R5’s documentation these legs are referred to as ‘segments’, a word more usually used to describe small sections on the transport network. Results contain information on the mode, waiting times, travel times and distances for each leg (or ‘segment’ in R5 documentation) and the trip geometry. Moreover, the `detailed_itineraries()` function can also return results for multiple route alternatives. Let’s see how this function works using a reproducible example.

obs. We only recommend using `detailed_itineraries()` in case you are interested in finding suboptimal alternative routes and/or need the geometry information of the outputs. If you only want to have route information detailed by trip segments, then we would strongly encourage you to use the `expanded_travel_time_matrix()` function.

# 2. Build routable transport network with `build_network()`

First, let’s load some libraries and build our multimodal transport network. In this example we’ll be using the a sample data set for the city of Porto Alegre (Brazil) included in `r5r`.

    # increase Java memory
    options(java.parameters = "-Xmx2G")

    # load libraries
    library(r5r)
    library(sf)
    library(ggplot2)
    library(data.table)

    # build a routable transport network with r5r
    data_path <- system.file("extdata/poa", package = "r5r")
    r5r_network <- build_network(data_path)

    # routing inputs
    mode <- c('walk', 'transit')
    max_trip_duration <- 60 # minutes

    # departure time
    departure_datetime <- as.POSIXct("13-05-2019 14:00:00",
                                     format = "%d-%m-%Y %H:%M:%S")

    # load origin/destination points
    poi <- fread(file.path(data_path, "poa_points_of_interest.csv"))

# 3. Detailed info by trip segment for multiple trip alternatives

In this example below, we want to know some alternative routes between a single origin/destination pair. To get multiple route alternatives, we need to set `shortest_path = FALSE`.

Note that in the example below we set `suboptimal_minutes = 8`. In this case, `r5r` will consider sub-optimal routes that arrive up to 8 minutes after the arrival of the optimal route.

    # set inputs
    origins <- poi[10,]
    destinations <- poi[12,]
    mode <- c("WALK", "TRANSIT")
    max_walk_time <- 60
    departure_datetime <- as.POSIXct("13-05-2019 14:00:00",
                                     format = "%d-%m-%Y %H:%M:%S")

    # calculate detailed itineraries
    det <- detailed_itineraries(
      r5r_network,
      origins = origins,
      destinations = destinations,
      mode = mode,
      departure_datetime = departure_datetime,
      max_walk_time = max_walk_time,
      suboptimal_minutes = 8,
      shortest_path = FALSE
      )

    head(det)

The output is a `data.frame sf` object, so we can easily visualize the results.

## 3.1 Visualize results

Static visualization with `ggplot2` package: To provide a geographic context for the visualization of the results in `ggplot2`, you can also use the `street_network_to_sf((` function to extract the OSM street network used in the routing.

    # extract OSM network
    street_net <- r5r::street_network_to_sf(r5r_network)

    # extract public transport network
    transit_net <- r5r::transit_network_to_sf(r5r_network)

    # plot
    fig <- ggplot() +
            geom_sf(data = street_net$edges, color='gray85') +
            geom_sf(data = subset(det, option <4), aes(color=mode)) +
            facet_wrap(.~option) +
            theme_void()

    fig

    # SAVE image
    ggsave(plot = fig, filename = 'inst/img/vig_detailed_ggplot.png',
           height = 5, width = 15, units='cm', dpi=200)

# 4. A few options:

### 4.1 Combining orings and destinations

- By default, `detailed_itineraries()` will query routes between the 1st origin to the 1st destination, then the 2nd origin to the 2nd destination, and so on. If you would like to query routes between all origins to all destinations you can simply set `all_to_all = TRUE`.

### 4.2 Keep geometry data in the output

- Be default, `detailed_itineraries()` will return the spatial geometry of results. To prevent retrieving this information you can simply set `drop_geometry = TRUE`.

# 5. Hack for frequency-based GTFS feeds

Please note that the `detailed_itineraries()` functions does not run on frequency-based GTFS feeds. A simple hack to overcome this problem is to convert your GTFS data from frequencies to time tables. This can be easily done using the `gtfstools` package. Here is how:

    library(gtfstools)

    # location of your frequency-based GTFS
    freq_gtfs_file <- system.file("extdata/spo/spo.zip", package = "r5r")

    # read GTFS data
    freq_gtfs <- gtfstools::read_gtfs(freq_gtfs_file)

    # convert from frequencies to time tables
    stop_times_gtfs <- gtfstools::frequencies_to_stop_times(freq_gtfs)

    # save it as a new GTFS.zip file
    gtfstools::write_gtfs(gtfs = stop_times_gtfs,
                          path = tempfile(pattern = 'stop_times_gtfs', fileext = '.zip'))

… and now you can use `r5r` on this `stop_times_gtfs.zip`.

### Cleaning up after usage

`r5r` objects are still allocated to any amount of memory previously set after they are done with their calculations. In order to remove an existing `r5r` object and reallocate the memory it had been using, we use the `stop_r5` function followed by a call to Java’s garbage collector, as follows:

    r5r::stop_r5(r5r_network)
    rJava::.jgc(R.gc = TRUE)

If you have any suggestions or want to report an error, please visit the package GitHub page.