Package: GInSARCorW
Type: Package
Title: GACOS InSAR Correction Workflow
Version: 1.15.8
Date: 2023-05-13
Author: Subhadip Datta
Maintainer: Subhadip Datta <subhadipdatta007@gmail.com>
Description: A workflow for correction of Differential Interferometric Synthetic Aperture Radar (DInSAR) atmospheric delay base on Generic Atmospheric Correction Online Service for InSAR (GACOS) data and correction algorithms proposed by Chen Yu. This package calculate the Both Zenith and LOS direction (User Depend). You have to just download GACOS product on your area and preprocessed D-InSAR unwrapped images. Cite those references and this package in your work, when using this framework.
    References: 
            Yu, C., N. T. Penna, and Z. Li (2017) <doi:10.1016/j.rse.2017.10.038>.
            Yu, C., Li, Z., & Penna, N. T. (2017) <doi:10.1016/j.rse.2017.10.038>.
            Yu, C., Penna, N. T., and Li, Z. (2017) <doi:10.1002/2016JD025753>.
License: GPL-3
URL:
        <https://subhadipdatta.wixsite.com/profile/post/ginsarcorw-gacos-insar-correction-workflow>
Repository: CRAN
Depends: raster, circular, sp
Encoding: UTF-8
RoxygenNote: 7.2.3
NeedsCompilation: no
Packaged: 2023-05-14 05:11:04 UTC; subha
Date/Publication: 2023-05-14 05:30:02 UTC
Built: R 4.6.0; ; 2026-06-20 02:57:31 UTC; windows
